{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["技术要求","工程量清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":7,"n_cols":5,"rows_kept":7,"merged":[[0,0,0,4],[5,0,5,1],[5,2,5,4],[6,0,11,4]],"flags":["formulas_cached_only"]}
["采购项目清单：三号楼16层西区和12层西区病房墙板改造"]
[]
["序号","项目名称","数量或规模","资金预算（万元）","资金来源"]
[1,"三号楼16层西区和12层西区病房墙板改造",null,28.19,"自筹"]
["合计",null,null,28.19]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：三号楼16层西区和12层西区病房墙板改造。\n二、项目用途说明：为满足医院需求。\n三、配置规格、附件及零配件（包括专用工具）： 1、详情见后附工程量清单；                                   \n2、墙面安装9mm厚，600mm宽，平缝，墙板材料为A级，防火等级B1级的竹木纤维集成墙板。\n                                    \n四、详细技术要求、参数及产品资料等：①、公司营业执照；②、法人签字并加盖公章的委托书；③、被委托人的身份证；④、失信被执行人、重大税收违法案件当事人名单、政府采购严重违法失信行为记录名单查询记录（“信用中国”及“中国政府采购网”查询记录）；⑤、近三年内参加招投标活动在经营活动中没有重大违法违纪记录的书面声明；⑥、须具有贰级以上（含贰级）（且符合资质证书承揽范围）装饰装修资质，拟派项目经理应具有二级或二级以上建筑工程专业注册建造师资格，且具备有效的安全生产考核合格证书。开标时，投标企业需提供上述证件的原件或复印件加公章由评委审验。\n\n五、售后服务条件及交货日期（或工期）：①、质量承诺；②、安全承诺：施工中做好施工组织，保证安全生产，防止人为的对场区管网的损坏。如有安全事故或对场区管网损坏，其造成的伤害事故及一切经济损失，由施工企业承担全责。"]

{"sheet":"工程量清单","index":1,"n_rows":1,"n_cols":1,"rows_kept":1,"merged":[[0,0,6,2]],"flags":["formulas_cached_only"]}
["一间病房内：\n1、拆除病房内原有插座、踢脚线、开关并恢复\n2、墙面安装竹木纤维集成墙板：（9mm厚，600mm宽，平缝，墙板材料为A级，防火等级B1级，国内知名品牌）\n南墙：3.54x0.87=3㎡\n北墙：5.13x2.47-1.2x2.1(门)-1.2x0.72(门)=9.2㎡  \n东墙：4.68x2.78-1.12x2.33（壁柜）=10.4㎡ \n西墙：5.15x2.78=14.3㎡ \n小计：36.9㎡\n3、竹木纤维顶角线23m,踢脚线20m\n\n三号楼16层西区共计16间病房\n三号楼12层西区共计16间病房\n总计：32间病房"]